Thorlabs Piezoelectric Deformable Mirror Application + TLDFM VXIPnP Instrument Driver - Readme
The Thorlabs Piezoelectric Deformable Mirror Application is used to operate Thorlabs DMP40 Deformable Mirror Instruments.

The TLDFM instrument driver modules provides programming support for Thorlabs DM series instruments.
The driver installs into your system's VXIPnP directory. This is typically 'C:\Program Files\IVI Foundation\VISA\WinNT' or 'C:\VXIPNP\WinNT'.
The instrument driver packages were created with National Instruments LabWindows/CVI 15.0.1. The LabVIEW version of these drivers were generated with LabVIEW Interface Generator for LabWindows/CVI Instrument Drivers 2.0 in conjunction with LabVIEW 8.5.

Note:
This software comes with additional software packages:
	- NI CVI runtime engine		http://www.ni.com/cvi
	- MS .Net Framework		http://www.microsoft.com/net
	- ComponentOne Studio WPF	http://www.componentone.com/SuperProducts/StudioWPF
	- Infragistics WPF Controls	http://www.infragistics.com

License:
The Piezoelectric Deformable Mirror Application software is copyright Ó 2019, Thorlabs GmbH. For license details please see file License.rtf in the applications installation directory.
The TLDFM instrument driver libraries are copyright Ó 2019, Thorlabs GmbH.

Supported Platforms:
This software was verified with the following platforms:
	- Windows 7		32-bit and 64-bit version
	- Windows 8.1	32-bit and 64-bit version
	- Windows 10		32-bit and 64-bit version

Piezoelectric Deformable Mirror Application Change log:
V1.0	Apr-2014		Internal Prototype
V2.0	Jul-2014		Initial Release
V2.0.1	Aug-2014		Minor Bug fixes
V2.1	Sep-2014	Introduced Status Bar, refactored control area and added an segment index overlay
V2.2	Oct-2014		Introduced Temperature Chart and Temperature logging
V2.3	Oct-2015		Introduced Arm relaxing and improved Control Loop Feature
V2.4	Apr-2017		Added DMP40-F01 Support
V2.6	Mar-2019		Removed NI-VISA Dependency, introduced NuGet-Packages and updated Specifications

TLDFM VXIpnp Instrument Driver Changelog:
V1.0	Jan-2014		Internal Prototype
V2.0	Jul-2014		Initial Release
V2.1	Aug-2014		Added Zernike Voltage Pattern Calculation
V2.2	Nov-2014		Added Resource functions
V2.3	Sep-2015	Zernike and Relax Function moved to extension driver
V2.4	Apr-2017		Added DMP40-F01 Support
V2.6	Mar-2019		Substituted TLvisa (NI-VISA Substitution) and introduced NuGet-Packages

TLDFMX VXIpnp Instrument Driver Changelog:
V1.0	Sep-2015	Initial Release
V2.0	Jun-2017		Introduced TLvisa (NI-VISA Substitution)
V2.6	Mar-2019		Introduced NuGet-Packages