Thorlabs PAX1000 Application + TLPAX VXIPnP Instrument Driver - Readme
The Thorlabs PAX1000 Application is used to operate Thorlabs PAX1000 Instruments.

The TLPAX driver installs to into your system's VXIPnP directory. This is typically 'C:\Program Files\IVI Foundation\VISA\WinNT' or '\C:\VXIPNP\WinNT'. The instrument driver package was created with National Instruments LabWindows/CVI 12.0.1. The LabVIEW version of this driver was generated with LabVIEW Interface Generator for LabWindows/CVI Instrument Drivers 2.0 in conjunction with LabVIEW 8.5. The .NET managed library was generated by the National Instruments Measurement Studio plug-in for Visual Studio.NET 2015.

Note:
This software comes with additional software packages:
	- NI VISA runtime engine		http://www.ni.com/visa
	- NI CVI runtime engine		http://www.ni.com/cvi
	- MS .Net Framework		http://www.microsoft.com/net

License:
The PAX1000 Application software is copyright Ó 2020, Thorlabs GmbH. For license details please see file License.rtf in the applications installation directory.
The TLPAX instrument driver libraries are copyright Ó 2020, Thorlabs GmbH.

Supported Platforms:
This software was verified with the following platforms:
	- Windows 7		32-bit and 64-bit version
	- Windows 8.1	         32-bit and 64-bit version
 	- Windows 10          32-bit and 64-bit version

PAX1000 Application Change log:

V1.2        Oct-2020
              - Default wavelength for PAX1000 metric devices is wrong. (Fixed)

V1.1	     Dec-2019	
                 -Phase-Difference was displayed radian and not degree. (Fixed)

V1.0	     Jun-29-2017	
                 Initial Release

TLPAX VXIpnp Instrument Driver Changelog:
V1.0	June-2017	Initial Release